<rdf:RDF

xmlns:rdf ="http://www.w3.org/1999/02/22-rdf-syntax-ns#"

xmlns:rdfs="http://www.w3.org/2000/01/rdf-schema#"

 xmlns:owl="http://www.w3.org/2002/07/owl#"

xmlns:sumo="http://reliant.teknowledge.com/DAML/SUMO.owl#"

xmlns:mid-level-ontology="http://reliant.teknowledge.com/DAML/Mid-level-ontology.owl#"

xmlns:geography="http://reliant.teknowledge.com/DAML/Geography.owl#"

xmlns:government="http://reliant.teknowledge.com/DAML/Government.owl#"

xmlns     ="http://reliant.teknowledge.com/DAML/Communications.owl#"

>


<!-- Copyright (c) 2003 Teknowledge Corporation. 

U.S. GOVERNMENT RIGHTS 
Use, duplication, or disclosure by the U.S. Government is subject to 
restrictions set forth in DFARS 227.7202-1(a) and 227.7202-3(a), 
DFARS 252.227-7013(c)(1)(ii), DFARS 252.227-7018, FAR 12.212(a), 
FAR 52.227-19, or FAR 52.227-14 (ALT III), as applicable. 

THIS SOFTWARE CONTAINS CONFIDENTIAL INFORMATION AND TRADE SECRETS OF 
TEKNOWLEDGE CORPORATION.  USE, DISCLOSURE, OR REPRODUCTION IS PROHIBITED 
WITHOUT THE PRIOR EXPRESS WRITTEN PERMISSION OF TEKNOWLEDGE CORPORATION. 

For academic and other licenses, contact kslicenses@teknowledge.com 

-->

<rdfs:Class rdf:ID= "AMRadioStation">

<rdfs:comment>AMRadioStation is the subclass of 

RadioStations that broadcast in an AMRadioFrequency.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="http://reliant.teknowledge.com/DAML/Mid-level-ontology.owl#RadioStation"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "AMRadioSystem">

<rdfs:comment>AMRadioSystem is the subclass of 

RadioSystems that use Radios, RadioStations, and other components 

that broadcast and receive in the AMRadioFrequency.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="#RadioSystem"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "AfricaONE">

<rdfs:comment>AfricaONE is a submarine FiberOpticCable link 

encircling the continent of Africa.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="#FiberOpticCable"/>

<rdfs:subClassOf rdf:resource ="#CommunicationSystem"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "Autodin">

<rdfs:comment>Autodin is the Automatic Digital Network of the 

UnitedStatesDepartmentOfDefense.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="#CommunicationSystem"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "Cable">

<rdfs:comment>Cable is a class of Devices that are strong 

lengths of wire, metal, or other material.  Cable includes materials 

used for supporting and securing physical loads, as well as 

ElectricalCable and CommunicationCables.  Electrical and 

communications cables require a complex composition, consisting of 

conductors protected by insulators.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="http://reliant.teknowledge.com/DAML/SUMO.owl#Device"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "CableTelevisionConnection">

<rdfs:comment>CableTelevisionConnection is the subclass of CommunicationDevices 

with protocols that enable a subscriber to connect her television to a 

CableTelevisionSystem.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="#CoaxialCable"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "CableTelevisionSystem">

<rdfs:comment>CableTelevisionSystem is the 

subclass of CommunicationSystems that disseminate Television signals 

to individual users by means of CoaxialCable connections.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="#CommunicationSystem"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "CellularTelephoneSystem">

<rdfs:comment>CellularTelephoneSystem is a 

subclass of TelephoneSystems in which the telephones are radio 

transceivers, with each instrument having its own private radio frequency 

and sufficient radiated power to reach the booster station in its area 

(cell), from which the telephone signal is fed to a TelephoneExchange.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="#TelephoneSystem"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "CitizensBandMobileRadio">

<rdfs:comment>CitizensBandMobileRadio is a 

subclass of TwoWayRadio sets that utilize frequencies set aside for public 

use in the UnitedStates.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="#TwoWayRadio"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "CitizensBandRadioMonitor">

<rdfs:comment>CitizensBandRadioMonitor is the 

subclass of $RadioReceivers that can receive radio broadcasts in the 

Citizens' Band (CB) frequencies.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="#RadioReceiver"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "CoaxialCable">

<rdfs:comment>CoaxialCable is a class of multichannel 

CommunicationCables that consist of two concentric conduction layers 

separated by insulation; a central conducting wire is surrounded by and 

insulated from a cylindrical conducting shell.  A large number of 

telephone channels can be made available within the insulated space by 

the use of a large number of carrier frequencies (WFB).</rdfs:comment>

<rdfs:subClassOf rdf:resource ="#CommunicationCable"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "CommunicationCable">

<rdfs:subClassOf rdf:resource ="#CommunicationLine"/>

<rdfs:comment>CommunicationCable is the subclass 

of Cables designed to serve as components in a CommunicationSystem.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="#Cable"/>

<rdfs:subClassOf rdf:resource ="http://reliant.teknowledge.com/DAML/Mid-level-ontology.owl#CommunicationDevice"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "CommunicationChannel">

<rdfs:comment>CommunicationChannel is the class 

whose instances are bands of frequencies of sufficient width for a single 

radio or television communication (MWO).</rdfs:comment>

<rdfs:subClassOf rdf:resource ="http://reliant.teknowledge.com/DAML/Mid-level-ontology.owl#CommunicationDevice"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "CommunicationFacility">

<rdfs:comment>CommunicationFacility is the 

subclass of StationaryArtifacts that consist of some type of 

CommunicationDevice serving as part of a CommunicationSystem.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="http://reliant.teknowledge.com/DAML/SUMO.owl#StationaryArtifact"/>

<rdfs:subClassOf rdf:resource ="http://reliant.teknowledge.com/DAML/Mid-level-ontology.owl#CommunicationDevice"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "CommunicationLine">

<rdfs:comment>CommunicationLine is the subclass of 

Device covering the broadest class of communication lines, including wire 

and cable, as well as fiber-optic lines.  Note that this represents wires 

or cables as whole objects; for lines in the sense of those (or those 

parts) carrying individual telephone communications, see TelephoneLine.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="http://reliant.teknowledge.com/DAML/SUMO.owl#Device"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "CommunicationOrganization">

<rdfs:comment>CommunicationOrganization is 

the subclass of Organizations that manage Communications over physical 

infrastructure owned or leased by the organization.  Such organizations 

may also produce and disseminate information, entertainment, or other 

content.  Cf. MediaOrganization.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="http://reliant.teknowledge.com/DAML/SUMO.owl#Organization"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "CommunicationSatellite">

<rdfs:comment>CommunicationSatellite is the 

subclass of ArtificialSatellites that serve as components of a 

CommunicationSystem.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="http://reliant.teknowledge.com/DAML/Mid-level-ontology.owl#ArtificialSatellite"/>

<rdfs:subClassOf rdf:resource ="http://reliant.teknowledge.com/DAML/Mid-level-ontology.owl#CommunicationDevice"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "CommunicationSystem">

<rdfs:comment>CommunicationSystem is a complex 

Physical system with various components, enabling communication (in some 

medium) between points in a specific area, whether local or worldwide.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="http://reliant.teknowledge.com/DAML/SUMO.owl#Object"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "ElectricalCable">

<rdfs:comment>ElectricalCable is the subclass of 

Cable consisting of heavy-duty insulated WireLine designed to transmit 

large amounts of electrical current.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="http://reliant.teknowledge.com/DAML/Mid-level-ontology.owl#WireLine"/>

<rdfs:subClassOf rdf:resource ="#Cable"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "ElectromagneticFrequency">

<rdfs:comment>ElectromagneticFrequency is the 

class of Attributes that describe the frequency band of a Device or 

of a RadiatingElectromagnetic process.  When applied to a device, the 

attribute indicates what kinds of frequencies it can receive or emit.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="http://reliant.teknowledge.com/DAML/SUMO.owl#InternalAttribute"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "ElectronicCommunication">

<rdfs:comment>ElectronicCommunication is the 

subclass of Communication processes that are accomplished using 

an electronic communication device or system as instrument.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="http://reliant.teknowledge.com/DAML/SUMO.owl#Communication"/>

<rdfs:subClassOf rdf:resource ="http://reliant.teknowledge.com/DAML/Mid-level-ontology.owl#ElectronicSignalling"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "ElectronicDevice">

<rdfs:comment>ElectronicDevice is the subclass of 

ElectricDevices that contain microchips or other solid-state electronic 

components.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="http://reliant.teknowledge.com/DAML/Mid-level-ontology.owl#ElectricDevice"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "FMRadioStation">

<rdfs:comment>FMRadioStation is the subclass of 

RadioStations that broadcast in an FMRadioFrequency.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="http://reliant.teknowledge.com/DAML/Mid-level-ontology.owl#RadioStation"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "FMRadioSystem">

<rdfs:comment>FMRadioSystem is the subclass of 

RadioSystems that use Radios, RadioStations, and other components 

that broadcast and receive in the FMRadioFrequency.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="#RadioSystem"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "Facsimile">

<rdfs:comment>Facsimile is the subclass of 

ContentBearingObjects that are facsimile reproductions created by 

TelefaxProcesses.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="http://reliant.teknowledge.com/DAML/SUMO.owl#ContentBearingObject"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "FiberOpticCable">

<rdfs:comment>FiberOpticCable is the subclass of 

CommunicationCables in which silica glass fiber serves as the conductor 

of pulses of light that constitute digital signals.  FiberOpticCable is 

a multichannel communications cable that uses a thread of optical glass 

fibers as a transmission medium in which the signal (voice, video, etc.) 

is in the form of a coded pulse of light (WFB).</rdfs:comment>

<rdfs:subClassOf rdf:resource ="#CommunicationCable"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "ISOInternetCountryCode">

<rdfs:comment>ISOInternetCountryCode is the class of two-letter codes maintained by 

the InternationalOrganizationForStandardization in the ISO 3166 Alpha-2 

list and used by the Internet Assigned Numbers Authority (IANA) to 

establish country-coded top-level domains (ccTLDs).</rdfs:comment>

<rdfs:subClassOf rdf:resource ="http://reliant.teknowledge.com/DAML/SUMO.owl#ContentBearingObject"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "InternetCafe">

<rdfs:comment>InternetCafe is a CommercialAgent and 

light Restaurant that provides its customers with access to the 

Internet either as a direct CommercialService or freely with the 

presumption that those on the premises are purchasing food or beverages.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="http://reliant.teknowledge.com/DAML/SUMO.owl#CommercialAgent"/>

<rdfs:subClassOf rdf:resource ="http://reliant.teknowledge.com/DAML/Mid-level-ontology.owl#Restaurant"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "InternetCommunication">

<rdfs:comment>InternetCommunication is the class 

of Communication processes that use the Internet, e.g., simple 

information lookup or complex real-time games played over the Internet.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="#ElectronicCommunication"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "InternetServiceProvider">

<rdfs:comment>InternetServiceProvider is the 

subclass of CommunicationOrganizations that provide access to the 

Internet.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="#CommunicationOrganization"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "Landline">

<rdfs:comment>Landline is the subclass of communication wire 

or cable of any sort that is installed on poles or buried in the ground 

(WFB).  This term is usually used to distinguish telephone connections over 

landlines from wireless communications.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="#CommunicationLine"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "MainTelephoneLine">

<rdfs:comment>MainTelephoneLine is the subclass of 

TelephoneLines that are connected directly to a PublicTelephoneSystem.  

Additional lines or extensions may be linked to a MainTelephoneLine 

within a private household or office.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="#TelephoneLine"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "Marecs">

<rdfs:comment>Marecs (Maritime European Communications 

Satellite) is the subclass of CommunicationSatellites used in the 

InmarsatOrganization system on lease from the European Space Agency.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="#CommunicationSatellite"/>

<rdfs:label>Marecs</rdfs:label>

<rdfs:label>Maritime European Communications Satellite</rdfs:label>

</rdfs:Class>



<rdfs:Class rdf:ID= "Marisat">

<rdfs:comment>Marisat is the subclass of 

CommunicationSatellites of the ComsatCorporation that participate in 

the InmarsatOrganization system.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="#CommunicationSatellite"/>

<rdfs:label>Marisat</rdfs:label>

</rdfs:Class>



<rdfs:Class rdf:ID= "MediaOrganization">

<rdfs:comment>MediaOrganization is the subclass 

of Organization for groups whose primary purpose is the production or 

dissemination of media content.  For organizations that enable 

Communication, see CommunicationOrganization.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="http://reliant.teknowledge.com/DAML/SUMO.owl#Organization"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "MicrowaveRadiation">

<rdfs:comment>MicrowaveRadiation is the subclass of 

RadiatingElectromagnetic processes in which the waves are of a very short 

length, between about one millimeter and one meter.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="http://reliant.teknowledge.com/DAML/SUMO.owl#RadiatingElectromagnetic"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "MicrowaveRadioRelay">

<rdfs:comment>MicrowaveRadioRelay is the class of 

transmissions of long distance telephone calls and television programs by 

highly directional radio microwaves that are received and sent on from one 

booster station to another on an optical path. (WFB)</rdfs:comment>

<rdfs:subClassOf rdf:resource ="#MicrowaveRadiation"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "MicrowaveRadioRelayStation">

<rdfs:comment>MicrowaveRadioRelayStation 

is the subclass of CommunicationFacility whose instances are stations 

that relay microwave communications.  See also MicrowaveRadioRelay.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="#CommunicationFacility"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "MobileCellPhone">

<rdfs:comment>MobileCellPhone is the subclass of 

Telephones that are used without an immediate connection to a 

MainTelephoneLine, because they connect via radio frequencies to 

local cell stations that relay the call to a TelephoneExchange.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="http://reliant.teknowledge.com/DAML/Mid-level-ontology.owl#Telephone"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "OrbitaTelevisionService">

<rdfs:comment>OrbitaTelevisionService is a 

Russian television service.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="#CommunicationOrganization"/>

<headquarters rdf:resource = "http://reliant.teknowledge.com/DAML/Mid-level-ontology.owl#Russia" />

</rdfs:Class>



<rdfs:Class rdf:ID= "PublicTelephoneSystem">

<rdfs:comment>PublicTelephoneSystem is the 

subclass of TelephoneSystems that connect users from multiple households, 

businesses, or agencies.  Note: 'Public' does not refer to ownership of 

the system, but to the fact that the system is not a private system being 

used only within one organization, but a public one that makes lines 

available to independent subscribers.  Ownership of the system itself may 

be either private or governmental.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="#TelephoneSystem"/>

</rdfs:Class>



<rdfs:Class rdf:about= "http://reliant.teknowledge.com/DAML/Mid-level-ontology.owl#RadioBroadcasting">

<rdfs:subClassOf rdf:resource ="#RadioCommunication"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "RadioCommunication">

<rdfs:comment>RadioCommunication is the 

subclass of ElectronicCommunication in which Radios are used as 

instruments of communication.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="#ElectronicCommunication"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "RadioReceiver">

<rdfs:comment>RadioReceiver is the subclass of Radio 

whose instances can only receive, but not send, radio communications.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="http://reliant.teknowledge.com/DAML/Mid-level-ontology.owl#Radio"/>

<sumo:disjoint rdf:resource = "#TwoWayRadio" />

</rdfs:Class>



<rdfs:Class rdf:ID= "RadioSystem">

<rdfs:comment>RadioSystem is the subclass of 

CommunicationSystem that consists of RadioStations, Radios, and 

other components that work together to make radio communication possible 

in a given area.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="#CommunicationSystem"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "RadioTelephone">

<rdfs:comment>RadioTelephone is the subclass of 

TwoWayRadios that are telephone-style handsets capable of radio 

communication on authorized frequencies.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="#TwoWayRadio"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "RadioTelephoneCommunication">

<rdfs:comment>RadioTelephoneCommunication 

is the process of two-way transmission and reception of sounds by 

broadcast radio on authorized frequencies using telephone handsets. (WFB)</rdfs:comment>

<rdfs:subClassOf rdf:resource ="#TelephoneCommunication"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "RadioTelephoneCommunicationSystem">

<rdfs:comment>RadioTelephoneCommunicationSystem is the subclass of 

TelephoneCommunicationSystems that use authorized radio frequencies 

for the transmission of telephone messages.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="#TelephoneSystem"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "RepeaterDevice">

<rdfs:comment>RepeaterDevice is a class of 

ElectronicDevices that are designed to receive, amplify, and relay an 

electronic signal.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="#ElectronicDevice"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "SatelliteCommunicationOrganization">

<rdfs:comment>SatelliteCommunicationOrganization is the subclass of 

CommunicationOrganizations that own or lease CommunicationSatellites 

and enable satellite Communication.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="#CommunicationOrganization"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "SatelliteCommunicationSystem">

<rdfs:comment>SatelliteCommunicationSystem 

is the subclass of CommunicationSystems that consist of two or more 

SatelliteEarthStations and at least one satellite, providing long 

distance transmission of voice, data, and television; the system usually 

serves as a trunk connection between telephone exchanges; if the earth 

stations are in the same country, it is a domestic system. (WFB)</rdfs:comment>

<rdfs:subClassOf rdf:resource ="#CommunicationSystem"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "SatelliteEarthStation">

<rdfs:comment>SatelliteEarthStation is the 

subclass of CommunicationFacility whose instances are equipped with 

a microwave radio transmitting and receiving antenna and required 

receiving and transmitting equipment for communicating with satellites. 

(WFB)</rdfs:comment>

<rdfs:subClassOf rdf:resource ="#CommunicationFacility"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "SatelliteLink">

<rdfs:comment>SatelliteLink is the class of radio 

Communication between a CommunicationSatellite and a 

SatelliteEarthStation, either one-way (e.g., down link from satellite 

to earth station, such as television receive-only transmission) or 

two-way (e.g., telephone channels).</rdfs:comment>

<rdfs:subClassOf rdf:resource ="http://reliant.teknowledge.com/DAML/SUMO.owl#Communication"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "ShortwaveRadioStation">

<rdfs:comment>ShortwaveRadioStation is the 

subclass of RadioStations that broadcast in a ShortwaveRadioFrequency.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="http://reliant.teknowledge.com/DAML/Mid-level-ontology.owl#RadioStation"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "ShortwaveRadioSystem">

<rdfs:comment>ShortwaveRadioSystem is the 

subclass of RadioSystems that use Radios, RadioStations, and other 

components that broadcast and receive in the ShortwaveRadioFrequency.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="#RadioSystem"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "SubmarineCommunicationCable">

<rdfs:comment>SubmarineCommunicationCable 

is a subclass of CommunicationCable especially designed for service 

under water. (WFB)</rdfs:comment>

<rdf:type rdf:resource = "#CommunicationCable"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "TelefaxProcess">

<rdfs:comment>TelefaxProcess is the subclass of 

Communication processes that are facsimile service between subscriber 

stations via the public switched telephone network or the international 

Datel network.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="#ElectronicCommunication"/>

<rdfs:subClassOf rdf:resource ="http://reliant.teknowledge.com/DAML/Mid-level-ontology.owl#Copying"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "TelegraphSystem">

<rdfs:comment>TelegraphSystem is the subclass of 

CommunicationSystems that are designed for unmodulated electric 

impulse transmission (WFB).</rdfs:comment>

<rdfs:subClassOf rdf:resource ="#CommunicationSystem"/>

</rdfs:Class>



<rdfs:Class rdf:about= "http://reliant.teknowledge.com/DAML/Mid-level-ontology.owl#Telephone">

<rdfs:subClassOf rdf:resource ="http://reliant.teknowledge.com/DAML/Mid-level-ontology.owl#CommunicationDevice"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "TelephoneChannel">

<rdfs:comment>TelephoneChannel is the subclass of 

CommunicationChannel consisting of a channel that can carry one 

telephone communication.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="#CommunicationChannel"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "TelephoneCommunication">

<rdfs:comment>TelephoneCommunication is the 

subclass of ElectronicCommunication in which Telephones are used as 

instruments of communication.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="#ElectronicCommunication"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "TelephoneExchange">

<rdfs:comment>TelephoneExchange is the subclass of 

CommunicationFacility for facilities where multiple TelephoneLines 

are connected in a TelephoneSystem.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="#CommunicationFacility"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "TelephoneLine">

<rdfs:comment>TelephoneLine is the class of physical 

media that carry single telephone signals for voice communication or 

electronic data transfer.  A single TelephoneLine is one wire or part 

of a wire or fiber optic cable needed for one such communication link.  

This generic notion of TelephoneLine covers any individual telephone 

line, whether a MainTelephoneLine, an extension line, or a line linked 

through a private exchange to the PublicTelephoneSystem.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="http://reliant.teknowledge.com/DAML/SUMO.owl#EngineeringConnection"/>

<rdfs:subClassOf rdf:resource ="#CommunicationLine"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "TelephoneSatellite">

<rdfs:comment>TelephoneSatellite is the subclass 

of CommunicationSatellites used for TelephoneCommunications.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="#CommunicationSatellite"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "TelephoneSystem">

<rdfs:comment>TelephoneSystem is the subclass of 

CommunicationSystem that consists of interconnected Telephones, 

TelephoneExchanges, and TelephoneLines or CommunicationSatellites, 

with any other needed components that work together to make telephonic 

communication possible from point to point in a given area.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="#CommunicationSystem"/>

</rdfs:Class>



<rdfs:Class rdf:about= "http://reliant.teknowledge.com/DAML/Mid-level-ontology.owl#Telephoning">

<rdfs:subClassOf rdf:resource ="http://reliant.teknowledge.com/DAML/Mid-level-ontology.owl#ElectronicSignalling"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "TelevisionChannel">

<rdfs:comment>TelevisionChannel is the subclass of 

CommunicationChannels designated for television communications.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="#CommunicationChannel"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "TelevisionChannelOrganization">

<rdfs:comment>TelevisionChannelOrganization 

is the subclass of CommunicationOrganizations that hold the rights to 

transmit programming on a particular TelevisionChannel.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="#CommunicationOrganization"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "TelevisionNetwork">

<rdfs:comment>TelevisionNetwork is the subclass of 

CommunicationSystems consisting of TelevisionStations that are linked 

electronically and managed or owned by one organization.  See also 

TelevisionNetworkOrganization.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="#CommunicationSystem"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "TelevisionNetworkOrganization">

<rdfs:comment>TelevisionNetworkOrganization 

is the subclass of CommunicationOrganizations that own or manage a 

TelevisionNetwork, including producing programs to disseminate over the 

physical network.  Television networks may be privately, publicly, or 

government-owned.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="#CommunicationOrganization"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "TelevisionRepeaterStation">

<rdfs:comment>TelevisionRepeaterStation is 

the subclass of TelevisionStations that rebroadcast the signal of one 

other TV station at all times (NMG).  Simplex repeaters rebroadcast the 

signal on the same frequency or channel as the received signal; translators 

rebroadcast the received signal on a different channel.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="http://reliant.teknowledge.com/DAML/Mid-level-ontology.owl#TelevisionStation"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "TelexService">

<rdfs:comment>TelexService is a communication service 

involving teletypewriters connected by wire through automatic exchanges.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="#CommunicationSystem"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "TransAtlanticTelephoneCable">

<rdfs:comment>TransAtlanticTelephoneCable 

is the subclass of high-capacity submarine coaxial telephone cables 

linking Europe with North America. (WFB)</rdfs:comment>

<rdfs:subClassOf rdf:resource ="#TelephoneLine"/>

<rdfs:subClassOf rdf:resource ="#CoaxialCable"/>

<rdfs:subClassOf rdf:resource ="#SubmarineCommunicationCable"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "TroposphericScatter">

<rdfs:comment>TroposphericScatter is a form of 

microwave radio transmission in which the troposphere is used to scatter 

and reflect a fraction of the incident radio waves back to earth; 

powerful, highly directional antennas are used to transmit and receive 

the microwave signals; reliable over-the-horizon communications are 

realized for distances up to 600 miles in a single hop; additional hops 

can extend the range of this system for very long distances. (WFB)</rdfs:comment>

<rdfs:subClassOf rdf:resource ="#MicrowaveRadiation"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "TrunkNetwork">

<rdfs:comment>TrunkNetwork is the subclass of 

CommunicationSystems consisting of networks of switching centers, 

connected by multichannel trunk lines.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="#CommunicationSystem"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "TwoWayRadio">

<rdfs:comment>TwoWayRadio is the subclass of Radio whose 

instances can both send and receive RadioCommunications.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="http://reliant.teknowledge.com/DAML/Mid-level-ontology.owl#Radio"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "URL">

<rdfs:comment>URL (Uniform Resource Locator, Universal Resource 

Locator) is the class of SymbolicStrings that are addresses for a 

Computer or a document on the Internet.</rdfs:comment>

<rdfs:subClassOf rdf:resource ="http://reliant.teknowledge.com/DAML/SUMO.owl#ContentBearingObject"/>

<rdfs:subClassOf rdf:resource ="http://reliant.teknowledge.com/DAML/SUMO.owl#SymbolicString"/>

</rdfs:Class>



<rdfs:Class rdf:ID= "WebSite">

<rdfs:comment>WebSite is the class of Internet addresses 

where an agent posts information.  Web sites may have restricted or 

unrestricted access (controlled via a server) and may consist of one or 

more 'pages' (individual addresses).</rdfs:comment>

<rdfs:subClassOf rdf:resource ="http://reliant.teknowledge.com/DAML/SUMO.owl#ContentBearingObject"/>

</rdfs:Class>



<owl:ObjectProperty   rdf:ID= "DomesticTelephoneSystemFn">

<rdfs:comment>(DomesticTelephoneSystemFn ?AREA) denotes the domestic TelephoneSystem 

of the GeopoliticalArea ?AREA.</rdfs:comment>

<rdf:type rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#UnaryFunction"/>

<rdfs:domain rdf:resource="http://reliant.teknowledge.com/DAML/SUMO.owl#GeopoliticalArea"/>

<rdfs:range rdf:resource = "#TelephoneSystem"/>

</owl:ObjectProperty>



<owl:ObjectProperty   rdf:ID= "InternationalTelephoneSystemFn">

<rdfs:comment>(InternationalTelephoneSystemFn ?AREA) denotes the international 

TelephoneSystem of the GeopoliticalArea ?AREA.</rdfs:comment>

<rdf:type rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#UnaryFunction"/>

<rdfs:domain rdf:resource="http://reliant.teknowledge.com/DAML/SUMO.owl#GeopoliticalArea"/>

<rdfs:range rdf:resource = "#TelephoneSystem"/>

</owl:ObjectProperty>



<owl:ObjectProperty   rdf:ID= "channelFrequency">

<rdfs:comment>(channelFrequency ?FREQ ?BAND) means 

that the frequency ?FREQ belongs to the CommunicationChannel ?BAND.</rdfs:comment>

<rdf:type rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#BinaryPredicate"/>

<rdf:type rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#SingleValuedRelation"/>

<rdfs:domain rdf:resource="http://reliant.teknowledge.com/DAML/SUMO.owl#TimeDependentQuantity"/>

<rdfs:range rdf:resource = "#CommunicationChannel"/>

</owl:ObjectProperty>



<owl:ObjectProperty   rdf:ID= "headquarters">

<rdfs:comment>(headquarters ?ORG ?PLACE) means that the 

Organization ?ORG has its headquarters located in or at the Object 

?PLACE.  The place may be either a GeographicArea or a Building.</rdfs:comment>

<rdf:type rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#BinaryPredicate"/>

<rdfs:domain rdf:resource="http://reliant.teknowledge.com/DAML/SUMO.owl#Organization"/>

<rdfs:range rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#Object"/>

<rdfs:subPropertyOf rdf:resource="http://reliant.teknowledge.com/DAML/SUMO.owl#partlyLocated"/>

</owl:ObjectProperty>



<owl:ObjectProperty   rdf:ID= "internetCountryCode">

<rdfs:comment>(internetCountryCode ?CODE ?AREA) 

means that the SymbolicString ?CODE, used in WebSite URLs and in 

Internet e-mail addresses, identifies users from the GeopoliticalArea 

?AREA.  See also ISOInternetCountryCode.</rdfs:comment>

<rdf:type rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#BinaryPredicate"/>

<rdfs:domain rdf:resource="http://reliant.teknowledge.com/DAML/SUMO.owl#SymbolicString"/>

<rdfs:range rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#GeopoliticalArea"/>

<rdfs:subPropertyOf rdf:resource="http://reliant.teknowledge.com/DAML/Government.owl#abbreviation"/>

</owl:ObjectProperty>



<owl:ObjectProperty   rdf:ID= "languageOfCommunication">

<rdfs:comment>(languageOfCommunication ?COMM ?LANGUAGE) means that 

the Communication event ?COMM is in the Language ?LANGUAGE.</rdfs:comment>

<rdf:type rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#BinaryPredicate"/>

<rdfs:domain rdf:resource="http://reliant.teknowledge.com/DAML/SUMO.owl#Communication"/>

<rdfs:range rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#Language"/>

</owl:ObjectProperty>



<owl:ObjectProperty   rdf:ID= "linksToWebsite">

<rdfs:comment>(linksToWebsite ?SITE1 ?SITE2) means that 

the WebSite ?SITE1 contains a link to the WebSite ?SITE2.</rdfs:comment>

<rdf:type rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#BinaryPredicate"/>

<rdf:type rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#TransitiveRelation"/>

<rdfs:domain rdf:resource="#WebSite"/>

<rdfs:range rdf:resource = "#WebSite"/>

</owl:ObjectProperty>



<owl:ObjectProperty   rdf:ID= "systemComponent">

<rdfs:comment>(systemComponent ?COMP ?SYSTEM) means 

that the Physical object ?COMP is a component of the Object ?SYSTEM.</rdfs:comment>

<rdf:type rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#BinaryPredicate"/>

<rdfs:domain rdf:resource="http://reliant.teknowledge.com/DAML/SUMO.owl#Physical"/>

<rdfs:range rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#Object"/>

<rdfs:subPropertyOf rdf:resource="http://reliant.teknowledge.com/DAML/SUMO.owl#component"/>

</owl:ObjectProperty>



<owl:ObjectProperty   rdf:ID= "telephoneCommunicationsModeInArea">

<rdfs:comment>(telephoneCommunicationsModeInArea ?AREA ?TYPE) means that in the 

GeopoliticalArea ?AREA, the domestic telephone system makes use of 

communications facilities of ?TYPE.</rdfs:comment>

<rdf:type rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#BinaryPredicate"/>

<rdfs:domain rdf:resource="http://reliant.teknowledge.com/DAML/SUMO.owl#GeographicArea"/>

<rdfs:range rdf:resource = "http://reliant.teknowledge.com/DAML/Mid-level-ontology.owl#CommunicationDevice"/>

</owl:ObjectProperty>



<owl:ObjectProperty   rdf:ID= "telephoneConnectionBetween">

<rdfs:comment>(telephoneConnectionBetween ?OBJ1 ?OBJ2) means that there is a 

telephone connection between the Entity ?OBJ1 and the Entity ?OBJ2.  

Note: The argument constraints are broad enough to cover places, people, 

organizations, and numbers (or strings) representing telephone numbers. 

For a predicate that specifies the system in which a connection is made, 

see telephoneSystemConnects.</rdfs:comment>

<rdf:type rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#BinaryPredicate"/>

<rdf:type rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#SymmetricRelation"/>

<rdfs:domain rdf:resource="http://reliant.teknowledge.com/DAML/SUMO.owl#Entity"/>

<rdfs:range rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#Entity"/>

</owl:ObjectProperty>



<owl:DatatypeProperty  rdf:ID= "totalCommunicationSatellitesForArea">

<rdfs:comment>(totalCommunicationSatellitesForArea ?AREA ?INTEGER) means that the 

GeographicArea ?AREA has a total of ?INTEGER number of 

CommunicationSatellites serving as parts of its CommunicationSystems.</rdfs:comment>

<rdf:type rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#BinaryPredicate"/>

<rdfs:domain rdf:resource="http://reliant.teknowledge.com/DAML/SUMO.owl#GeographicArea"/>

<rdfs:range rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#NonnegativeInteger"/>

</owl:DatatypeProperty>



<owl:DatatypeProperty  rdf:ID= "totalInternetHouseholdsInArea">

<rdfs:comment>(totalInternetHouseholdsInArea ?AREA ?COUNT) means that in the 

GeographicArea ?AREA, the number of households that have a connection 

to the internet is ?COUNT.</rdfs:comment>

<rdf:type rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#BinaryPredicate"/>

<rdfs:domain rdf:resource="http://reliant.teknowledge.com/DAML/SUMO.owl#GeographicArea"/>

<rdfs:range rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#NonnegativeInteger"/>

</owl:DatatypeProperty>



<owl:DatatypeProperty  rdf:ID= "totalInternetServiceProvidersForArea">

<rdfs:comment>(totalInternetServiceProvidersForArea ?AREA ?COUNT) means that in the 

GeographicArea ?AREA, the number of InternetServiceProviders is 

?COUNT.</rdfs:comment>

<rdf:type rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#BinaryPredicate"/>

<rdfs:domain rdf:resource="http://reliant.teknowledge.com/DAML/SUMO.owl#GeographicArea"/>

<rdfs:range rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#NonnegativeInteger"/>

</owl:DatatypeProperty>



<owl:DatatypeProperty  rdf:ID= "totalInternetUsersInArea">

<rdfs:comment>(totalInternetUsersInArea ?AREA ?COUNT) means that in the 

GeographicArea ?AREA, the number of people who access the internet, 

on either a regular or occasional basis, is ?COUNT.</rdfs:comment>

<rdf:type rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#BinaryPredicate"/>

<rdfs:domain rdf:resource="http://reliant.teknowledge.com/DAML/SUMO.owl#GeographicArea"/>

<rdfs:range rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#NonnegativeInteger"/>

</owl:DatatypeProperty>



<owl:DatatypeProperty  rdf:ID= "totalMobileCellularTelephonesInArea">

<rdfs:comment>(totalMobileCellularTelephonesInArea ?AREA ?NUMBER) means that in the 

GeographicArea ?AREA, there are ?NUMBER of MobileCellPhones in use.</rdfs:comment>

<rdf:type rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#BinaryPredicate"/>

<rdfs:domain rdf:resource="http://reliant.teknowledge.com/DAML/SUMO.owl#GeographicArea"/>

<rdfs:range rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#NonnegativeInteger"/>

</owl:DatatypeProperty>



<owl:DatatypeProperty  rdf:ID= "totalRadioReceiversInArea">

<rdfs:comment>(totalRadioReceiversInArea ?AREA ?COUNT) means that in the 

GeographicArea ?AREA, the number of RadioReceivers is ?COUNT.</rdfs:comment>

<rdf:type rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#BinaryPredicate"/>

<rdfs:domain rdf:resource="http://reliant.teknowledge.com/DAML/SUMO.owl#GeographicArea"/>

<rdfs:range rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#NonnegativeInteger"/>

</owl:DatatypeProperty>



<owl:DatatypeProperty  rdf:ID= "totalSatelliteEarthStationsBySystemInArea">

<rdfs:comment>(totalSatelliteEarthStationsBySystemInArea ?AREA ?NETWORK ?COUNT) means 

that the number of SatelliteEarthStations used by telephone systems of 

the GeographicArea ?AREA to monitor the CommunicationSystem (or 

CommunicationOrganization) ?NETWORK, is ?COUNT.</rdfs:comment>

<rdf:type rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#BinaryPredicate"/>

<rdfs:domain rdf:resource="http://reliant.teknowledge.com/DAML/SUMO.owl#GeographicArea"/>

<rdfs:range rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#Object"/>

<rdfs:range rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#NonnegativeInteger"/>

</owl:DatatypeProperty>



<owl:DatatypeProperty  rdf:ID= "totalSatelliteEarthStationsInArea">

<rdfs:comment>(totalSatelliteEarthStationsInArea ?AREA ?COUNT) means that in the 

GeographicArea ?AREA, the number of SatelliteEarthStations is ?COUNT.</rdfs:comment>

<rdf:type rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#BinaryPredicate"/>

<rdfs:domain rdf:resource="http://reliant.teknowledge.com/DAML/SUMO.owl#GeographicArea"/>

<rdfs:range rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#NonnegativeInteger"/>

</owl:DatatypeProperty>



<owl:DatatypeProperty  rdf:ID= "totalTelephoneLinesInArea">

<rdfs:comment>(totalTelephoneLinesInArea ?AREA ?NUMBER) means that in the 

GeographicArea ?AREA, there are ?NUMBER of MainTelephoneLines in use.</rdfs:comment>

<rdf:type rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#BinaryPredicate"/>

<rdfs:domain rdf:resource="http://reliant.teknowledge.com/DAML/SUMO.owl#GeographicArea"/>

<rdfs:range rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#NonnegativeInteger"/>

</owl:DatatypeProperty>



<owl:DatatypeProperty  rdf:ID= "totalTelevisionCableSystemsInArea">

<rdfs:comment>(totalTelevisionCableSystemsInArea ?AREA ?COUNT) means that in the 

GeographicArea ?AREA, the number of CableTelevisionSystems is ?COUNT.</rdfs:comment>

<rdf:type rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#BinaryPredicate"/>

<rdfs:domain rdf:resource="http://reliant.teknowledge.com/DAML/SUMO.owl#GeographicArea"/>

<rdfs:range rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#NonnegativeInteger"/>

</owl:DatatypeProperty>



<owl:DatatypeProperty  rdf:ID= "totalTelevisionRepeaterStationsInArea">

<rdfs:comment>(totalTelevisionRepeaterStationsInArea ?AREA ?COUNT) means that in the 

GeographicArea ?AREA, the number of TelevisionStations is ?COUNT.  

In the CIA World Fact Book, the number of repeater stations is given 

in addition to the total number of separate broadcast stations.  See also, 

totalTelevisionStationsInArea.</rdfs:comment>

<rdf:type rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#BinaryPredicate"/>

<rdfs:domain rdf:resource="http://reliant.teknowledge.com/DAML/SUMO.owl#GeographicArea"/>

<rdfs:range rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#NonnegativeInteger"/>

</owl:DatatypeProperty>



<owl:DatatypeProperty  rdf:ID= "totalTelevisionSetsInArea">

<rdfs:comment>(totalTelevisionSetsInArea ?AREA ?COUNT) means that in the 

GeographicArea ?AREA, the number of Television sets is ?COUNT.</rdfs:comment>

<rdf:type rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#BinaryPredicate"/>

<rdfs:domain rdf:resource="http://reliant.teknowledge.com/DAML/SUMO.owl#GeographicArea"/>

<rdfs:range rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#NonnegativeInteger"/>

</owl:DatatypeProperty>



<owl:DatatypeProperty  rdf:ID= "totalTelevisionStationsInArea">

<rdfs:comment>(totalTelevisionStationsInArea ?AREA ?COUNT) means that in the 

GeopoliticalArea ?AREA, the number of TelevisionStations is ?COUNT.  

In the CIA World Fact Book, this entry gives the total number of separate 

broadcast stations (WFB), with repeater stations summed separately.  See 

also, totalTelevisionRepeaterStationsInArea.</rdfs:comment>

<rdf:type rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#BinaryPredicate"/>

<rdfs:domain rdf:resource="http://reliant.teknowledge.com/DAML/SUMO.owl#GeographicArea"/>

<rdfs:range rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#NonnegativeInteger"/>

</owl:DatatypeProperty>



<owl:ObjectProperty   rdf:ID= "wavelength">

<rdfs:comment>(wavelength ?WAVE ?AMOUNT) means that 

the Motion process ?WAVE has a LengthMeasure of ?AMOUNT.</rdfs:comment>

<rdf:type rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#BinaryPredicate"/>

<rdf:type rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#AsymmetricRelation"/>

<rdfs:domain rdf:resource="http://reliant.teknowledge.com/DAML/SUMO.owl#Motion"/>

<rdfs:range rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#LengthMeasure"/>

<rdfs:subPropertyOf rdf:resource="http://reliant.teknowledge.com/DAML/SUMO.owl#measure"/>

</owl:ObjectProperty>



<owl:ObjectProperty   rdf:ID= "websiteURLOfAgent">

<rdfs:comment>(websiteURLOfAgent ?URL ?AGENT) means 

that the WebSite with the address ?URL belongs to the CognitiveAgent 

?AGENT.</rdfs:comment>

<rdf:type rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#BinaryPredicate"/>

<rdfs:domain rdf:resource="http://reliant.teknowledge.com/DAML/SUMO.owl#SymbolicString"/>

<rdfs:range rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#CognitiveAgent"/>

</owl:ObjectProperty>



<rdf:Description rdf:ID= "AMRadioFrequency">

<rdfs:comment>AMRadioFrequency is the Attribute 

describing radio frequencies in the range of 540 to 1800 kilohertz.</rdfs:comment>

<rdf:type rdf:resource = "#ElectromagneticFrequency"/>

</rdf:Description>



<rdf:Description rdf:ID= "Arabsat">

<rdfs:comment>Arabsat is the Arab Satellite Communications 

Organization based in RiyadhSaudiArabia.</rdfs:comment>

<rdf:type rdf:resource = "#SatelliteCommunicationOrganization"/>

<rdfs:label>Arabsat</rdfs:label>

<rdfs:label>Arab Satellite Communications Organization</rdfs:label>

<headquarters rdf:resource = "http://reliant.teknowledge.com/DAML/Government.owl#RiyadhSaudiArabia" />

</rdf:Description>



<rdf:Description rdf:ID= "CEPT">

<rdfs:comment>CEPT is the Conference Europeanne des Posts et 

Telecommunication.</rdfs:comment>

<rdf:type rdf:resource = "#CommunicationOrganization"/>

<rdfs:label>Conference Europeanne des Posts et Telecommunication</rdfs:label>

<headquarters rdf:resource = "http://reliant.teknowledge.com/DAML/Mid-level-ontology.owl#ParisFrance" />

<sumo:relatedInternalConcept rdf:resource = "#GSM" />

</rdf:Description>



<rdf:Description rdf:ID= "CentralAmericanMicrowaveSystem">

<rdfs:comment>CentralAmericanMicrowaveSystem is a CommunicationSystem that is 

a trunk microwave radio relay system that links the countries of Central 

America and Mexico with each other.</rdfs:comment>

<rdf:type rdf:resource = "#CommunicationSystem"/>

</rdf:Description>



<rdf:Description rdf:ID= "ComsatCorporation">

<rdfs:comment>ComsatCorporation is the Communications 

Satellite Corporation of the UnitedStates.</rdfs:comment>

<rdf:type rdf:resource = "#SatelliteCommunicationOrganization"/>

<rdfs:label>Comsat</rdfs:label>

<rdfs:label>Communications Satellite Corporation</rdfs:label>

<headquarters rdf:resource = "http://reliant.teknowledge.com/DAML/Mid-level-ontology.owl#UnitedStates" />

</rdf:Description>



<rdf:Description rdf:ID= "DefenseSwitchedNetwork">

<rdfs:comment>DefenseSwitchedNetwork 

is the basic general-purpose, switched voice network of the 

DefenseCommunicationsSystem of the UnitedStates DepartmentOfDefense.</rdfs:comment>

<rdf:type rdf:resource = "#CommunicationSystem"/>

<rdfs:label>Defense Switched Network</rdfs:label>

</rdf:Description>



<rdf:Description rdf:ID= "EutelsatOrganization">

<rdfs:comment>EutelsatOrganization is the European Telecommunications 

Satellite Organization, based in ParisFrance.</rdfs:comment>

<rdf:type rdf:resource = "#SatelliteCommunicationOrganization"/>

<rdfs:label>Eutelsat</rdfs:label>

<rdfs:label>European Telecommunications Satellite Organization</rdfs:label>

<headquarters rdf:resource = "http://reliant.teknowledge.com/DAML/Mid-level-ontology.owl#ParisFrance" />

</rdf:Description>



<rdf:Description rdf:ID= "FMRadioFrequency">

<rdfs:comment>FMRadioFrequency is the Attribute 

describing radio frequencies in the range of 88 to 108 megahertz.</rdfs:comment>

<rdf:type rdf:resource = "#ElectromagneticFrequency"/>

</rdf:Description>



<rdf:Description rdf:ID= "GSM">

<rdfs:comment>GSM is a global system for mobile (cellular) 

communications devised by the Groupe Special Mobile of the pan-European 

standardization organization, Conference Europeanne des Posts et 

Telecommunications (CEPT) in 1982.</rdfs:comment>

<rdf:type rdf:resource = "#CommunicationSystem"/>

</rdf:Description>



<rdf:Description rdf:ID= "HighFrequency">

<rdfs:comment>HighFrequency is the Attribute 

describing radio frequencies in the range of 3,000 to 30,000 kilohertz.</rdfs:comment>

<rdf:type rdf:resource = "#ElectromagneticFrequency"/>

<sumo:successorAttribute rdf:resource = "#VeryHighFrequency" />

</rdf:Description>



<rdf:Description rdf:ID= "InmarsatOrganization">

<rdfs:comment>InmarsatOrganization is the 

International Mobile Satellite Organization (LondonUK); provider of 

global mobile satellite communications for commercial, distress, and safety 

applications at sea, in the air, and on land.</rdfs:comment>

<rdf:type rdf:resource = "#SatelliteCommunicationOrganization"/>

<rdfs:label>Inmarsat</rdfs:label>

<rdfs:label>International Mobile Satellite Organization</rdfs:label>

<headquarters rdf:resource = "http://reliant.teknowledge.com/DAML/Mid-level-ontology.owl#LondonUK" />

</rdf:Description>



<rdf:Description rdf:ID= "IntelsatOrganization">

<rdfs:comment>IntelsatOrganization is the 

International Telecommunications Satellite Organization, based in 

WashingtonDC.</rdfs:comment>

<rdf:type rdf:resource = "#SatelliteCommunicationOrganization"/>

<rdfs:label>Intelsat</rdfs:label>

<rdfs:label>International Telecommunications Satellite Organization</rdfs:label>

<headquarters rdf:resource = "http://reliant.teknowledge.com/DAML/Mid-level-ontology.owl#WashingtonDC" />

</rdf:Description>



<rdf:Description rdf:ID= "InternationalTelecommunicationsUnion">

<rdfs:comment>InternationalTelecommunicationsUnion (ITU) is the 

CommunicationOrganization that runs Medarabtel.</rdfs:comment>

<rdf:type rdf:resource = "#CommunicationOrganization"/>

<rdfs:label>International Telecommunication Union</rdfs:label>

<mid-level-ontology:financialAsset rdf:resource = "#Medarabtel" />

</rdf:Description>



<rdf:Description rdf:ID= "Internet">

<rdf:type rdf:resource = "#CommunicationSystem"/>

<rdfs:comment>The Internet is a CommunicationSystem

for the rapid delivery of information between computers.</rdfs:comment>

</rdf:Description>



<rdf:Description rdf:ID= "IntersputnikOrganization">

<rdfs:comment>IntersputnikOrganization is the 

International Organization of Space Communications, based in MoscowRussia; 

first established in the former Soviet Union and the East European countries, 

it is now marketing its services worldwide with earth stations in 

NorthAmerica, Africa, and East Asia.</rdfs:comment>

<rdf:type rdf:resource = "#SatelliteCommunicationOrganization"/>

<rdfs:label>Intersputnik</rdfs:label>

<rdfs:label>International Organization of Space Communications</rdfs:label>

<headquarters rdf:resource = "http://reliant.teknowledge.com/DAML/Government.owl#MoscowRussia" />

</rdf:Description>



<rdf:Description rdf:ID= "Medarabtel">

<rdfs:comment>Medarabtel is the Middle East Telecommunications 

Project of the International Telecommunications Union (ITU), providing a 

modern telecommunications network, primarily by microwave radio relay, linking 

Algeria, Djibouti, Egypt, Jordan, Libya, Morocco, Saudi Arabia, Somalia, 

Sudan, Syria, Tunisia, and Yemen; it was initially started in Morocco in 

1970 by the Arab Telecommunications Union (ATU) and was known at that time as 

the Middle East Mediterranean Telecommunications Network. (WFB)</rdfs:comment>

<rdf:type rdf:resource = "#CommunicationSystem"/>

<rdfs:label>Medarabtel</rdfs:label>

<rdfs:label>Middle East Telecommunications Project</rdfs:label>

</rdf:Description>



<rdf:Description rdf:ID= "MedarabtelCountry">

<rdfs:comment>MedarabtelCountry is the group of 

Nations that are linked by the Medarabtel telecommunications system.</rdfs:comment>

<rdf:type rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#Group"/>

<sumo:member rdf:resource = "http://reliant.teknowledge.com/DAML/Geography.owl#Algeria" />

<sumo:member rdf:resource = "http://reliant.teknowledge.com/DAML/Geography.owl#Djibouti" />

<sumo:member rdf:resource = "http://reliant.teknowledge.com/DAML/Geography.owl#Egypt" />

<sumo:member rdf:resource = "http://reliant.teknowledge.com/DAML/Geography.owl#Jordan" />

<sumo:member rdf:resource = "http://reliant.teknowledge.com/DAML/Geography.owl#Libya" />

<sumo:member rdf:resource = "http://reliant.teknowledge.com/DAML/Geography.owl#Morocco" />

<sumo:member rdf:resource = "http://reliant.teknowledge.com/DAML/Geography.owl#SaudiArabia" />

<sumo:member rdf:resource = "http://reliant.teknowledge.com/DAML/Geography.owl#Somalia" />

<sumo:member rdf:resource = "http://reliant.teknowledge.com/DAML/Geography.owl#Sudan" />

<sumo:member rdf:resource = "http://reliant.teknowledge.com/DAML/Geography.owl#Syria" />

<sumo:member rdf:resource = "http://reliant.teknowledge.com/DAML/Geography.owl#Tunisia" />

<sumo:member rdf:resource = "http://reliant.teknowledge.com/DAML/Geography.owl#Yemen" />

</rdf:Description>



<rdf:Description rdf:ID= "NonsecureInternetProtocolRouterNetwork">

<rdfs:comment>NonsecureInternetProtocolRouterNetwork (NIPRNET) is an 

InternetServiceProvider run by the UnitedStatesDepartmentOfDefense.</rdfs:comment>

<rdf:type rdf:resource = "#InternetServiceProvider"/>

</rdf:Description>



<rdf:Description rdf:ID= "NordicMobileTelephone">

<rdfs:comment>NordicMobileTelephone (NMT) is an 

analog cellular telephone system that was developed jointly by the 

national telecommunications authorities of the Nordic countries (Denmark, 

Finland, Iceland, Norway, and Sweden). (WFB)</rdfs:comment>

<rdf:type rdf:resource = "#CellularTelephoneSystem"/>

<sumo:relatedInternalConcept rdf:resource = "http://reliant.teknowledge.com/DAML/Geography.owl#Denmark" />

<sumo:relatedInternalConcept rdf:resource = "http://reliant.teknowledge.com/DAML/Geography.owl#Finland" />

<sumo:relatedInternalConcept rdf:resource = "http://reliant.teknowledge.com/DAML/Geography.owl#Iceland" />

<sumo:relatedInternalConcept rdf:resource = "http://reliant.teknowledge.com/DAML/Geography.owl#Norway" />

<sumo:relatedInternalConcept rdf:resource = "http://reliant.teknowledge.com/DAML/Mid-level-ontology.owl#Sweden" />

</rdf:Description>



<rdf:Description rdf:ID= "OrbitaTelephoneNetwork">

<rdfs:comment>OrbitaTelephoneNetwork is a 

packet-switched digital telephone network.</rdfs:comment>

<rdf:type rdf:resource = "#TelephoneSystem"/>

</rdf:Description>



<rdf:Description rdf:ID= "PanAmSatCorporation">

<rdfs:comment>PanAmSatCorporation is the PanAmSat 

Corporation, based in Greenwich, Connecticut (U.S.).</rdfs:comment>

<rdf:type rdf:resource = "http://reliant.teknowledge.com/DAML/SUMO.owl#Corporation"/>

<rdf:type rdf:resource = "#SatelliteCommunicationOrganization"/>

<headquarters rdf:resource = "http://reliant.teknowledge.com/DAML/Mid-level-ontology.owl#UnitedStates" />

</rdf:Description>



<rdf:Description rdf:about= "http://reliant.teknowledge.com/DAML/Mid-level-ontology.owl#Russia">

<sumo:possesses rdf:resource = "#OrbitaTelephoneNetwork" />

<sumo:possesses rdf:resource = "#StatsionerSystem" />

</rdf:Description>



<rdf:Description rdf:ID= "ShortwaveRadioFrequency">

<rdfs:comment>ShortwaveRadioFrequency is the 

Attribute describing radio frequencies (from 1.605 to 30 megahertz) that 

fall above the commercial broadcast band and are used for communication 

over long distances.</rdfs:comment>

<rdf:type rdf:resource = "#ElectromagneticFrequency"/>

</rdf:Description>



<rdf:Description rdf:ID= "SolidaridadSystem">

<rdfs:comment>SolidaridadSystem is Mexico's system 

of geosynchronous CommunicationSatellites used for international 

telecommunications in the Western Hemisphere.</rdfs:comment>

<rdf:type rdf:resource = "#CommunicationSystem"/>

</rdf:Description>



<rdf:Description rdf:ID= "StatsionerSystem">

<rdfs:comment>StatsionerSystem is Russia's 

geostationary system for satellite telecommunications.</rdfs:comment>

<rdf:type rdf:resource = "#SatelliteCommunicationSystem"/>

</rdf:Description>



<rdf:Description rdf:ID= "SuperHighFrequency">

<rdfs:comment>SuperHighFrequency is the 

Attribute describing radio frequencies in the range of 3,000 to 30,000 

megahertz.</rdfs:comment>

<rdf:type rdf:resource = "#ElectromagneticFrequency"/>

</rdf:Description>



<rdf:Description rdf:ID= "UltraHighFrequency">

<rdfs:comment>UltraHighFrequency is the Attribute 

that describes radio frequency in the range of 300 to 3,000 megahertz.</rdfs:comment>

<rdf:type rdf:resource = "#ElectromagneticFrequency"/>

<sumo:successorAttribute rdf:resource = "#SuperHighFrequency" />

</rdf:Description>



<rdf:Description rdf:about= "http://reliant.teknowledge.com/DAML/Mid-level-ontology.owl#UnitedStatesDepartmentOfDefense">

<sumo:possesses rdf:resource = "#Autodin" />

<sumo:possesses rdf:resource = "#DefenseSwitchedNetwork" />

<sumo:possesses rdf:resource = "#NonsecureInternetProtocolRouterNetwork" />

</rdf:Description>



<rdf:Description rdf:ID= "VeryHighFrequency">

<rdfs:comment>VeryHighFrequency is the Attribute 

that describes radio frequency in the range of 30 to 300 megahertz.</rdfs:comment>

<rdf:type rdf:resource = "#ElectromagneticFrequency"/>

<sumo:successorAttribute rdf:resource = "#UltraHighFrequency" />

</rdf:Description>



<rdf:Description rdf:ID= "WorldWideWeb">

<rdfs:comment>WorldWideWeb is part of the Internet 

that uses hypertext links to navigate the system.</rdfs:comment>

<rdf:type rdf:resource = "#CommunicationSystem"/>

<sumo:part rdf:resource = "#Internet" />

</rdf:Description>





</rdf:RDF>
